PAPER TITLE IS LEFT ALIGNED HERE

(Font to be 10 point, Times New Roman, throughout)

**1st Author Name**

Company Position

Company

City, State, Country

**3rd Author Name**

Company Position

Company

City, State, Country

**2nd Author Name**

Company Position

Company

City, State, Country

**4th Author Name**

Company Position

Company

City, State, Country, etc.

First author biography information. The picture is to be 0.8 inch by 1 inch, with text wrapping around the right side and under the picture (under the picture, if text extends beyond bottom of picture). Authors 2-4 follow the same format, in order.

# ABSTRACT

The possible negative or positive impact of annular seal on rotordynamics of compressors and steam turbines is discussed. The nature of destabilizing forces that can be developed by see-through and interlocking labyrinths is discussed.

# INTRODUCTION

The first task of an annular seal is the restriction of leakage flowrate between a rotating shaft and a stationary housing. As it turns out, annular gas seals can also have a significant impact on dynamic characteristics of compressors and turbines.

# MAIN HEADINGS

Main headings are 10 point font, bold and capitalized with two lines of space above and one line of space below. Use the “Heading 1” style for main headings.

## Second Level Headings

Second level headings are 10 point font, bold and italicized with one line of space above and no additional lines of space below. Use the “Heading 2” style for second level headings.

### Third Level Headings

Third level headings are 10 point font and italicized with one line of space above and no additional lines of space below. Use the “Heading 3” style for second level headings.

#### Fourth Level Headings

Fourth level headings are 10 point font, italicized, and indented one ¼ inch tab with one line of space above and no additional lines of space below.

High-pressure compressors can use either the flow-through or the back-to-back designs of Figure 1. In the through-flow design, gas enters from the left and proceeds directly from impeller to impeller.

The most important seal parameters include the following:

* Diameter
* Length
* Clearance
* Tooth geometry
  + Pitch
  + Height

An equation is described by Equation (1)

(1)

where;

force vector,

mass,

acceleration vector,

gravitational conversion factor,

# CONCLUSIONS

The initial (narrow) view of labyrinth seals as bad actors that caused rotordynamic instability problems has broadened today, to the view that annular seals can be used to remarkably improve rotordynamic response and stability characteristics of turbomachinery.

# NOMENCLATURE

*A* = Area (L2)

*r* = Radius (L)

*γ* = Area ratio (-)

HPOTP = High pressure oxygen turbopump

SSME = Space shuttle main engine

TOR = Teeth on rotor

# APPENDIX A

Appendix A begins here. Appendix A begins here. Appendix A begins here. Appendix A begins here.

# REFERENCES

Childs, D., Elrod, D., and Hale. K., 1988, Rotordynamic Coefficient and Leakage Test Results for Interlock and Tooth-on-Stator Labyrinth Seals, ASME Paper Number 88-GT-87, Gas Turbine Conference.

Ehrich, F. F., 1992, *Handbook of Rotordynamics*, New York, New York: McGraw-Hill.

Vance, J. M. And Li, J., 1996, Test Results of a New Damper Seal for Vibration Reduction in Turbomachinery, ASME Transactions, Journal of Engineering for Gas Turbines and Power, *118*, pp. 843-846.

**ACKNOWLEDGEMENTS**

Acknowledgements go here. Acknowledgements go here. Acknowledgements go here. Acknowledgements go here.